**DEALER PRE-DELIVERY INSPECTION HAY TEDDERS**

DEALER: Date of Inspection:

MODEL: Inspector:

SERIAL#:

|  |  |  |  |
| --- | --- | --- | --- |
| Criteria | Yes | No | N/A |
| Is oil in the center gearbox at the proper level |  |  |  |
| Is grease in the rotor gearboxes |  |  |  |
| Tines have been installed with the black tine on the right side in alternating pattern with Grey tine on the left side. Also the long leg of the tine is towards the outside. |  |  |  |
| Lug nuts torqued to 70ft/lbs |  |  |  |
| Bolts and nuts have been visually checked for any loose or missing hardware |  |  |  |
| The transport Latch Arms have been installed (6102 only) see ops manual for dealer setup instructions. |  |  |  |
| All guards and shielding are installed around rotating shafts. |  |  |  |
| The timing of the tedding arms is accurate (arms are equally spaced) |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |